Matrix Height Adjustable Basin - NBS specification
Client: [Insert Client]
N13
Sanitary appliances and fittings
Clauses - Not Used
Products
310 Wash basins generally

1.	Basin
1.1.	Manufacturer:  Multicare Medical Ltd
1.1.1.	Contact details
1.1.1.1.	Address:  Progress House
	Jacknell Road
	Dodwells Bridge Industrial Estate
	Hinckley
	Leicestershire
	LE10 3BS
1.1.1.2.	Telephone:  0800 298 6000
1.1.1.3.	Web:  multicaremedical.co.uk
1.1.1.4.	Email:  sales@multicaremedical.co.uk
1.1.2.	Product reference:  Matrix Height Adjustable Basin
1.2.	Form:  Wall mounted, wheelchair friendly, height adjustable wash basin.
1.3.	Operation:  Electric height adjustment by inset front push-button controls.
1.4.	Height adjustment range:  670 - 970 mm.
1.5.	Width:  780 - 1200 mm, subject to selected basin size.
1.6.	Width variations:  900 mm or 1200 mm.
1.7.	Basin options:
1.7.1.	Square or curved front basin.
1.7.2.	Medium curved front basin with integrated handrails.
1.7.3.	Overflow:  Available where specified.
1.8.	Taps:
1.8.1.	TMV3 long lever taps with built-in thermostatic protection; or
1.8.2.	Infra-red, gesture-operated, thermostatically controlled taps.
1.9.	Safety:  Safety stop to reduce crushing risk during adjustment.
1.10.	Finish:  White protective cover to conceal plumbing and electrics.
1.11.	Materials:  Aluminium basin lifter and high quality damage resistant materials.
1.12.	Services:  Installation, commissioning, maintenance, servicing and training available from Multicare.
1.13.	Warranty:  1 year.

Specifier note: Confirm final basin size, front profile, tap option, overflow requirement, wall structure, services and setting-out with Multicare prior to installation.
Multicare Medical Ltd




